ECE 480
Pre-Proposal

Ethernet Integrity Analyzer
Sponsored By Texas Instruments

Design Team 7:
Sponsor: Jim Reinhart
Facilitator: Dr. Donnie Reinhard

Ahmed Alsinan- Documentation Prep.
Andrew Christopherson- Web Design
Sedat Gur- Lab Coordinator
Mark Jones- Manager
Brian Schulte- Presentation Prep.


Executive Summary
Due to the expanding use of Ethernet technology, the need for a troubleshooting device is becoming more of a necessity. To fulfill this need, we intend to put Texas Instruments at the forefront of this industry by creating an Ethernet Integrity Analyzer designed around existing TI technologies including the TLK100 Ethernet transceiver. This handheld device will have the capabilities of performing a series of cable diagnostics over an Ethernet line. These diagnostics will detect and locate faults such as, cable damage, water ingress, and manufacturing flaws. In addition, the device supports the relatively new technology of Power-over-Ethernet which will decrease power consumption and lower cost of operation.
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Ethernet has become one of the most popular and widely deployed network technologies in the world. In today's increasingly complex internet and client-server environments, the need for Ethernet Analyzers is becoming more essential for network operation and maintenance. ECE 480 Design Team 7 will design and develop a handheld analyzer for Ethernet networks. Our Ethernet Integrity Analyzer (EIA) will automatically execute a diagnostic suite, and perform integrity checks when plugged into a standard RJ-45 Ethernet port. The EIA will display the results of the tests by its on-board color touch-screen display and can optionally tag and store the results in a data log to be later uploaded to a host PC for off-line analysis. The EIA is powered from one of three sources: Power-over-Ethernet if detected on the link, a DC input supply or, if neither of the line sources are detected, batteries.           

[bookmark: _Toc253923101]Background

Currently, there are a limited amount of diagnostic tools for Ethernet Networks. Many of the current tools require significant knowledge of networks and can take a significant amount of time to accurately diagnose. TI has a number of existing technologies that we will incorporate to create a new network analyzing tool that will be intuitive and handheld.  The most significant TI product to be incorporated is the TLK100 Ethernet PHY, a physical layer device that offers three capabilities Time Domain Reflectometry (TDR), Active Link Cable Diagnostic (ALCD) and Digital Spectrum Analyzer (DSA).  A new technology being used is Power-over-Ethernet which will be incorporated through the Texas Insturment's TPS2376 PoE PD Controller. Another highlighted TI hardware technology is the ARM Cortex M3 MCU. The software will be developed using StellarisWare which is used to program the microcontroller in C++. The software will also be written using IAR embedded workbench which is a development environment for programming ARM-based embedded applications.   

[bookmark: _Toc253923102]Objectives or Design Specifications

	Our design will diagnose a RJ-45 Ethernet line to determine its integrity. The Stellaris® LM3S9B96 Development Board (shown in Figure 1) presents a platform for developing systems around the advanced capabilities of the LM3S9B96 ARM® Cortex™-M3 based microcontroller. The LM3S9B96 is a member of the Stellaris Tempest-Class microcontroller family which contains capabilities such as 80MHz clock speeds, an External Peripheral Interface (EPI) and Audio I2C interfaces. To support these features, the DK-LM3S9B96 includes a rich set of peripherals found on other Stellaris boards. This development kit will lead us to design and test the implementation of our Ethernet Integrity Analyzer. The kit also provides some features such as, Controller Area Network (CAN), 10/100 BaseT Ethernet, 1MB flash memory and LCD monitor. 
 (
Figure 1:  Development Board
)   
				                     
	The Development Board is supplied by 4.75-5.25 V dc voltage from USB cable, USB micro-B cable (USBs connected to a PC) or DC power jack. Power-over-Ethernet (PoE) technology will be used when power is detected by the TPS2376-H PoE PD. The power used from the Ethernet line will be converted to +5V DC in order to be used to power the Development Board. To have a rechargeable battery system with a wall adapter, the bq24070 Single-Chip LI-ION Charge and Power-Path Mgmt IC will be used. Once this power has been converted to +5V DC, it can be logically combined with the PoE using Option 1 illustrated in Figure 2. This will allow for switching between the rechargeable battery system with wall adapter and the PoE. The EIA will be designed such that the PoE will be the primary power supply with the batteries and wall adapter as an alternate. The battery will supply power when no other power source is detected. 
 (
Figure 2: 
Power-over-Ethernet 
Schematic
)
	The TLK100 will be used to provide the connection between the Media Independent Interface (MII) and the Media Access Controller (MAC). The mixed-signal processing is used by the TLK100 to equalize, recover data, and to correct error. The TLK100 is able to handle large amounts of interference and noise, creating a robust system. It has the capability to run Time Domain compliance Reflectometry (TDR), Active Link Cable Diagnostic (ALCD), and Digital Spectrum Analyzer (DSA). Time Domain Reflectometry (TDR) will be used for locating errors in the cable as well as measuring the length of the cable. By analyzing reflections of a test pulse the TDR will be able to calculate impedances throughout the line and the locations of those impedances. Active Link Cable Diagnostic (ALCD) is capable of measuring the overall cable length with even higher accuracy than the TDR. Finally the Digital Spectrum Analyzer (DSA) will be used to find the magnitude of the frequency response (119.2 Hz Resolution).

 (
Figure 
3
: 
)	
	This single port transceiver will allow us to perform cable diagnostics. The TLK100 uses Time Domain Reflectrometry (TDR) to determine the quality of the cables, connectors, and terminations. Also, TLK100 supports Active Link Cable Diagnostic. This offers a passive method to estimate the cable length during the active link. The other diagnostic our design will cover is analysis of the channel frequency response. The TLK100 offers a unique capability of Digital Spectrum Analyzer. 
Below in figure 4 is a block diagram of the entire project.
 (
Figure 4: Ethernet Integrity Analyzer Block Diagram
)
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For this project, receiving parts in a timely manner is one of the biggest issues that we have that could prevent the project from being completed on time. Some core components have long delivery times. A broken part could end up slowing down the development for weeks if there is not a backup on hand. Creating a solution that is small enough to fit in a handheld devices is also a concern, since some components come with unneeded features, increasing their complexity and size.
[bookmark: _Toc253923105]Project Management Plan

	Name
	Non-Technical Role
	Technical Role

	Ahmed Alsinan
	Documentation Preparation
	POE to battery switching

	Andrew Christopherson
	Web Design
	Programming microcontroller/LCD display

	Sedat Gur
	Lab Coordinator
	DC/DC conversion

	Mark Jones
	Manager
	Programming TLK100 Ethernet PHY

	Brian Schulte
	Presentation Preparation
	Battery/AC Power Implementation


	
	Week
	Tasks

	Week 1: 1/11 – 1/17
	· Meet with team
· Receive Project Description
· Meet with Facilitator

	Week 2: 1/18 – 1/24
	· Begin Research on project
· Conference call with sponsor

	Week 3: 1/25 – 1/31
	· Request critical parts from TI

	Week 4: 2/1 – 2/7
	· Pre-Proposal Due
· Request additional parts

	Week 5: 2/8 – 2/14
	· Voice of Customer Due

	Week 6: 2/15 – 2/21
	· Receive Development Kit
· Final Proposal Due
· Oral Presentation

	Week 7: 2/22 – 2/28
	· Begin coding touch display
· Work on interface between microcontroller and Ethernet PHY
· FAST Diagram Due
· Design Day Program Page Due

	Week 8: 3/1 – 3/7
	· Begin work on Power Over Ethernet controller
· Code Ethernet PHY to run diagnostics

	Spring Break: 3/8 – 3/14
	· Time Off

	Week 9: 3/15 – 3/21
	· Progress Report #1
· Demo of project
· Complete implementation of switching between POE and batteries 

	Week 10: 3/22 – 3/28
	· Student technical lecture
· Implement Passive mode for analyzer

	Week 11: 3/29 – 4/4
	· Individual application notes due

	Week 12: 4/5 – 4/11
	· Progress Report #2
· Second demo of porject

	Week 13: 4/12 – 4/18
	· Design Issues Paper
· Working model of Ethernet Analyzer

	Week 14: 4/19 – 4/25
	· Finish Poster and Final Report
· Practice Design Day Presentation

	Week 15: 4/26 – 5/2
	· Design Day
· Turn in Engineering Notebooks
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Budget

While TI will be providing most of the parts needed for this project, making it so our group has very little control over the cost of the final design, we will try to create a rough estimate of what  the cost of the final design might be. Our 500 dollar budget will be used for various minor tools and parts as they are needed.
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