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Power Arduino Arduino IDE | Processing | Linear | Actuator | Mechanical | Force Sensing |Printed Circuit| Wire | Selecting
Importance | Source | Microcontroller [Programming | Interface | Actuators | Control Linkage |Resistors (FSR) Board Harness | Pedal

User adjustable number of
detents 5 1 9 9 9 3 9 3 3 1
User defined detent force S 9 9 9 9 3 9 3 9 3 1
USB connectivity 4 9 3 3 3 1
Cross-platform use (Mac, PC,
Linux, etc.) 3 9 9 9
Physical position sustainability
(no return to center) 4 1 1 9 3 9 1
Low cost to manufacture 2 3 3 3 3 3 1
Inherent user interface 2 3 9 3
Easily mountable 2 3 1 9 9 1 1 3

Totals 50 175 133 147 68 165 90 69 50 26 14





